# Blast Pot Preventive Maintenance

Preventive maintenance checklist based on manufacturer recommendations once every 6 months.

Checklist:

* Inspect pressure vessel for corrosion or cracks (internally & externally)
* Check and clean metering valve and moisture separator.
* Ensure deadman system functions correctly.
* Inspect plunger and doughnut seal condition
* Drain any moisture from the bottom drain valve.
* Inspect blast hose for wear and damage.
* Check couplings and gaskets for leaks.
* Inspect and test auto air valve operation (check diaphragm)
* Replace copper mufflers (auto air valve)
* Test blowdown system and venting.