# Carbon Monoxide Detector Preventive Maintenance

Preventive maintenance checklist based on manufacturer recommendations and monthly intervals where applicable.

Checklist:

* Perform calibration using certified calibration gas.
* Inspect and replace 9V batteries if low battery light is on.
* Test audible and visual alarms weekly.
* Check hose and fittings for leaks or blockages.
* Clean and inspect sample inlet filter regularly.
* Verify flow rate is between 50–100 cc/min.
* Replace filter elements when indicators turn orange.
* Clean lens and LEDs as needed.