# Daily Maintenance Checklist - Compressor 900

* ☐ Check engine oil level
* ☐ Check compressor oil level
* ☐ Check coolant level
* ☐ Drain water from fuel/water separator (If applicable)
* ☐ Check battery connections for sulfating
* ☐ Check for oil or coolant leaks on floor and inside compressor
* ☐ Conduct general inspection of machine (damage, scrapes, tires, etc)