# Compressor 900 Preventive Maintenance

Preventive maintenance checklist based on manufacturer recommendations and 500-hour intervals where applicable.

Checklist:

* Check engine oil level and refill as needed.
* Inspect and clean air filter; replace if dirty.
* Check compressor oil level; change every 500 or 1,000 hours.
* Inspect and clean cooling system (pressure wash radiator)
* Check belt tension and wear.
* Drain water from fuel tank and separator (if applicable)
* Check battery terminals and electrolyte levels.
* Clean or replace fuel filters every 500 hours.
* Grease wheel bearings (if trailer-mounted).
* Check trailer lights