**Daily Maintenance Checklist - Compressor**

☐ Check engine oil level

☐ Check compressor oil level

☐ Check coolant level

☐ Check for oil or coolant leaks on floor and inside compressor

☐ Conduct general inspection of machine (damage, scrapes, tires, etc)

**Daily Maintenance Checklist - Vacuum**

☐ Check engine oil and coolant levels

☐ Drain water from the separator tank

☐ Conduct general inspection of machine (damage, scrapes, tires, etc)

☐ Check for oil, fuel, and coolant leaks on floor

**Daily Maintenance Checklist – Moisture Separator**

☐ Inspect the moisture separator housing for any visible damage or corrosion.

☐ Open the drain valve to remove accumulated water and contaminants.

☐ Check air motor oil level.

**Daily Maintenance Checklist - In-Line Carbon Monoxide Detector**

☐ Verify detector is powered and indicator lights are functional.

**Daily Maintenance Checklist – Blasting Pot**

☐ Ensure pot if fully depressurized

☐ Perform general inspection for damage, scrapes, etc.

☐ Drain moisture from separator