# Ford F550 Flatbed Truck (Diesel) Preventive Maintenance

Preventive maintenance checklist based on manufacturer recommendations and 500-hour intervals where applicable.

Checklist:

* Change engine oil and filter every 7,500 miles or 500 hours.
* Inspect and top off coolant and other fluid levels.
* Check transmission and brake fluids.
* Test battery voltage and clean terminals.
* Inspect air filter and replace if dirty.
* Check tire pressure and alignment.
* Inspect suspension and steering components.
* Examine exhaust system for leaks.
* Rotate tires as needed.
* Inspect lighting, horn, and wipers.