# Moisture Separator Preventive Maintenance

Preventive maintenance checklist based on manufacturer recommendations and 500-hour intervals where applicable.

Checklist:

* Inspect for rust, cracks, or damage.
* Drain accumulated moisture daily from the bottom valve.
* Check and clean internal mesh or coalescing elements.
* Verify airflow is unobstructed.
* Ensure valves are functional and sealing properly.
* Inspect for oil carryover; service filter if present.
* Lubricate valve stems if applicable.
* Check for air leaks in fittings and connectors.
* Check dessicant level and replace as needed (if applicable)