# Vacuum Preventive Maintenance

Preventive maintenance checklist based on manufacturer recommendations and 500-hour intervals where applicable.

Checklist:

* Check and change engine oil every 250 hours.
* Replace baghouse filters
* Inspect and clean blower filter element.
* Grease blower and drive components.
* Inspect and tighten all hose clamps.
* Clean vacuum relief valve.
* Inspect and replace blower oil as needed.
* Check condition and tension of belts.
* Check for vacuum leaks and repair as necessary.
* Clean the air filter on the diesel engine.
* Check hydraulic oil level if equipped.