# Daily Maintenance Checklist - Bulk Pot

* ☐ Ensure pot if fully depressurized
* ☐ Perform general inspection for damage, scrapes, etc.
* ☐ Drain moisture from separator