# Isuzu Box Truck Preventive Maintenance

Preventive maintenance checklist based on manufacturer recommendations and 500-hour intervals where applicable.

Checklist:

* Check and change engine oil and filter every 10,000 miles or 400 hours.
* Inspect brake system and fluid level.
* Check tire pressure and tread wear.
* Inspect all lights and warning indicators.
* Check and refill coolant level.
* Inspect battery condition and terminals.
* Inspect belts and hoses.
* Check transmission fluid level.
* Inspect air filter and replace if necessary.
* Lubricate chassis components as required.