# Daily Maintenance Checklist – Moisture Separator

☐ Inspect the moisture separator housing for any visible damage or corrosion.

☐ Open the drain valve to remove accumulated water and contaminants.

☐ Ensure that the automatic or manual drain mechanism is working correctly.

☐ Check air motor oil level.