# Daily Maintenance Checklist - Vacuum

* ☐ Check engine oil and coolant levels
* ☐ Drain water from the separator tank
* ☐ Inspect hydraulic oil level
* ☐ Conduct general inspection of machine (damage, scrapes, tires, etc)
* ☐ Check for oil, fuel, and coolant leaks on floor